    /*
     * jchuff.c
     *
     * Copyright (C) 1991-1997, Thomas G. Lane.
     * Modified 2006-2020 by Guido Vollbeding.
     * This file is part of the Independent JPEG Group's software.
     * For conditions of distribution and use, see the accompanying README file.
     *
     * This file contains Huffman entropy encoding routines.
     * Both sequential and progressive modes are supported in this single module.
     *
     * Much of the complexity here has to do with supporting output suspension.
     * If the data destination module demands suspension, we want to be able to
     * back up to the start of the current MCU.  To do this, we copy state
     * variables into local working storage, and update them back to the
     * permanent JPEG objects only upon successful completion of an MCU.
     *
     * We do not support output suspension for the progressive JPEG mode, since
     * the library currently does not allow multiple-scan files to be written
     * with output suspension.
     */

    #define JPEG_INTERNALS
    #include "jinclude.h"
    #include "jpeglib.h"

    /* The legal range of a DCT coefficient is
     *  -1024 .. +1023  for 8-bit data;
     * -16384 .. +16383 for 12-bit data.
     * Hence the magnitude should always fit in 10 or 14 bits respectively.
     */

    #if BITS_IN_JSAMPLE == 8
    #define MAX_COEF_BITS 10
    #else
    #define MAX_COEF_BITS 14
    #endif

    /* Derived data constructed for each Huffman table */

    typedef struct {
      unsigned int ehufco[256];	/* code for each symbol */
      char ehufsi[256];		/* length of code for each symbol */
      /* If no code has been allocated for a symbol S, ehufsi[S] contains 0 */
    } c_derived_tbl;

    /* Expanded entropy encoder object for Huffman encoding.
     *
     * The savable_state subrecord contains fields that change within an MCU,
     * but must not be updated permanently until we complete the MCU.
     */

    typedef struct {
      INT32 put_buffer;		/* current bit-accumulation buffer */
      int put_bits;			/* # of bits now in it */
      int last_dc_val[MAX_COMPS_IN_SCAN]; /* last DC coef for each component */
    } savable_state;

    /* This macro is to work around compilers with missing or broken
     * structure assignment.  You'll need to fix this code if you have
     * such a compiler and you change MAX_COMPS_IN_SCAN.
     */

    #ifndef NO_STRUCT_ASSIGN
    #define ASSIGN_STATE(dest,src)  ((dest) = (src))
    #else
    #if MAX_COMPS_IN_SCAN == 4
    #define ASSIGN_STATE(dest,src)  \
    	((dest).put_buffer = (src).put_buffer, \
    	 (dest).put_bits = (src).put_bits, \
    	 (dest).last_dc_val[0] = (src).last_dc_val[0], \
    	 (dest).last_dc_val[1] = (src).last_dc_val[1], \
    	 (dest).last_dc_val[2] = (src).last_dc_val[2], \
    	 (dest).last_dc_val[3] = (src).last_dc_val[3])
    #endif
    #endif

    typedef struct {
      struct jpeg_entropy_encoder pub; /* public fields */

      savable_state saved;		/* Bit buffer & DC state at start of MCU */

      /* These fields are NOT loaded into local working state. */
      unsigned int restarts_to_go;	/* MCUs left in this restart interval */
      int next_restart_num;		/* next restart number to write (0-7) */

      /* Pointers to derived tables (these workspaces have image lifespan) */
      c_derived_tbl * dc_derived_tbls[NUM_HUFF_TBLS];
      c_derived_tbl * ac_derived_tbls[NUM_HUFF_TBLS];

      /* Statistics tables for optimization */
      long * dc_count_ptrs[NUM_HUFF_TBLS];
      long * ac_count_ptrs[NUM_HUFF_TBLS];

      /* Following fields used only in progressive mode */

      /* Mode flag: TRUE for optimization, FALSE for actual data output */
      boolean gather_statistics;

      /* next_output_byte/free_in_buffer are local copies of cinfo->dest fields.
       */
      JOCTET * next_output_byte;	/* => next byte to write in buffer */
      size_t free_in_buffer;	/* # of byte spaces remaining in buffer */
      j_compress_ptr cinfo;		/* link to cinfo (needed for dump_buffer) */

      /* Coding status for AC components */
      int ac_tbl_no;		/* the table number of the single component */
      unsigned int EOBRUN;		/* run length of EOBs */
      unsigned int BE;		/* # of buffered correction bits before MCU */
      char * bit_buffer;		/* buffer for correction bits (1 per char) */
      /* packing correction bits tightly would save some space but cost time... */
    } huff_entropy_encoder;

    typedef huff_entropy_encoder * huff_entropy_ptr;

    /* Working state while writing an MCU (sequential mode).
     * This struct contains all the fields that are needed by subroutines.
     */

    typedef struct {
      JOCTET * next_output_byte;	/* => next byte to write in buffer */
      size_t free_in_buffer;	/* # of byte spaces remaining in buffer */
      savable_state cur;		/* Current bit buffer & DC state */
      j_compress_ptr cinfo;		/* dump_buffer needs access to this */
    } working_state;

    /* MAX_CORR_BITS is the number of bits the AC refinement correction-bit
     * buffer can hold.  Larger sizes may slightly improve compression, but
     * 1000 is already well into the realm of overkill.
     * The minimum safe size is 64 bits.
     */

    #define MAX_CORR_BITS  1000	/* Max # of correction bits I can buffer */

    /* IRIGHT_SHIFT is like RIGHT_SHIFT, but works on int rather than INT32.
     * We assume that int right shift is unsigned if INT32 right shift is,
     * which should be safe.
     */

    #ifdef RIGHT_SHIFT_IS_UNSIGNED
    #define ISHIFT_TEMPS	int ishift_temp;
    #define IRIGHT_SHIFT(x,shft)  \
    	((ishift_temp = (x)) < 0 ? \
    	 (ishift_temp >> (shft)) | ((~0) << (16-(shft))) : \
    	 (ishift_temp >> (shft)))
    #else
    #define ISHIFT_TEMPS
    #define IRIGHT_SHIFT(x,shft)	((x) >> (shft))
    #endif

    /*
     * Compute the derived values for a Huffman table.
     * This routine also performs some validation checks on the table.
     */

    LOCAL(void)
    jpeg_make_c_derived_tbl (j_compress_ptr cinfo, boolean isDC, int tblno,
    			 c_derived_tbl ** pdtbl)
    {
      JHUFF_TBL *htbl;
      c_derived_tbl *dtbl;
      int p, i, l, lastp, si, maxsymbol;
      char huffsize[257];
      unsigned int huffcode[257];
      unsigned int code;

      /* Note that huffsize[] and huffcode[] are filled in code-length order,
       * paralleling the order of the symbols themselves in htbl->huffval[].
       */

      /* Find the input Huffman table */
      if (tblno < 0 || tblno >= NUM_HUFF_TBLS)
        ERREXIT1(cinfo, JERR_NO_HUFF_TABLE, tblno);
      htbl =
        isDC ? cinfo->dc_huff_tbl_ptrs[tblno] : cinfo->ac_huff_tbl_ptrs[tblno];
      if (htbl == NULL)
        htbl = jpeg_std_huff_table((j_common_ptr) cinfo, isDC, tblno);

      /* Allocate a workspace if we haven't already done so. */
      if (*pdtbl == NULL)
        *pdtbl = (c_derived_tbl *) (*cinfo->mem->alloc_small)
          ((j_common_ptr) cinfo, JPOOL_IMAGE, SIZEOF(c_derived_tbl));
      dtbl = *pdtbl;

      /* Figure C.1: make table of Huffman code length for each symbol */

      p = 0;
      for (l = 1; l <= 16; l++) {
        i = (int) htbl->bits[l];
        if (i < 0 || p + i > 256)	/* protect against table overrun */
          ERREXIT(cinfo, JERR_BAD_HUFF_TABLE);
        while (i--)
          huffsize[p++] = (char) l;
      }
      huffsize[p] = 0;
      lastp = p;

      /* Figure C.2: generate the codes themselves */
      /* We also validate that the counts represent a legal Huffman code tree. */

      code = 0;
      si = huffsize[0];
      p = 0;
      while (huffsize[p]) {
        while (((int) huffsize[p]) == si) {
          huffcode[p++] = code;
          code++;
        }
        /* code is now 1 more than the last code used for codelength si; but
         * it must still fit in si bits, since no code is allowed to be all ones.
         */
        if (((INT32) code) >= (((INT32) 1) << si))
          ERREXIT(cinfo, JERR_BAD_HUFF_TABLE);
        code <<= 1;
        si++;
      }

      /* Figure C.3: generate encoding tables */
      /* These are code and size indexed by symbol value */

      /* Set all codeless symbols to have code length 0;
       * this lets us detect duplicate VAL entries here, and later
       * allows emit_bits to detect any attempt to emit such symbols.
       */
      MEMZERO(dtbl->ehufsi, SIZEOF(dtbl->ehufsi));

      /* This is also a convenient place to check for out-of-range
       * and duplicated VAL entries.  We allow 0..255 for AC symbols
       * but only 0..15 for DC.  (We could constrain them further
       * based on data depth and mode, but this seems enough.)
       */
      maxsymbol = isDC ? 15 : 255;

      for (p = 0; p < lastp; p++) {
        i = htbl->huffval[p];
        if (i < 0 || i > maxsymbol || dtbl->ehufsi[i])
          ERREXIT(cinfo, JERR_BAD_HUFF_TABLE);
        dtbl->ehufco[i] = huffcode[p];
        dtbl->ehufsi[i] = huffsize[p];
      }
    }

    /* Outputting bytes to the file.
     * NB: these must be called only when actually outputting,
     * that is, entropy->gather_statistics == FALSE.
     */

    /* Emit a byte, taking 'action' if must suspend. */
    #define emit_byte_s(state,val,action)  \
    	{ *(state)->next_output_byte++ = (JOCTET) (val);  \
    	  if (--(state)->free_in_buffer == 0)  \
    	    if (! dump_buffer_s(state))  \
    	      { action; } }

    /* Emit a byte */
    #define emit_byte_e(entropy,val)  \
    	{ *(entropy)->next_output_byte++ = (JOCTET) (val);  \
    	  if (--(entropy)->free_in_buffer == 0)  \
    	    dump_buffer_e(entropy); }

    LOCAL(boolean)
    dump_buffer_s (working_state * state)
    /* Empty the output buffer; return TRUE if successful, FALSE if must suspend */
    {
      struct jpeg_destination_mgr * dest = state->cinfo->dest;

      if (! (*dest->empty_output_buffer) (state->cinfo))
        return FALSE;
      /* After a successful buffer dump, must reset buffer pointers */
      state->next_output_byte = dest->next_output_byte;
      state->free_in_buffer = dest->free_in_buffer;
      return TRUE;
    }

    LOCAL(void)
    dump_buffer_e (huff_entropy_ptr entropy)
    /* Empty the output buffer; we do not support suspension in this case. */
    {
      struct jpeg_destination_mgr * dest = entropy->cinfo->dest;

      if (! (*dest->empty_output_buffer) (entropy->cinfo))
        ERREXIT(entropy->cinfo, JERR_CANT_SUSPEND);
      /* After a successful buffer dump, must reset buffer pointers */
      entropy->next_output_byte = dest->next_output_byte;
      entropy->free_in_buffer = dest->free_in_buffer;
    }

    /* Outputting bits to the file */

    /* Only the right 24 bits of put_buffer are used; the valid bits are
     * left-justified in this part.  At most 16 bits can be passed to emit_bits
     * in one call, and we never retain more than 7 bits in put_buffer
     * between calls, so 24 bits are sufficient.
     */

    INLINE
    LOCAL(boolean)
    emit_bits_s (working_state * state, unsigned int code, int size)
    /* Emit some bits; return TRUE if successful, FALSE if must suspend */
    {
      /* This routine is heavily used, so it's worth coding tightly. */
      register INT32 put_buffer;
      register int put_bits;

      /* if size is 0, caller used an invalid Huffman table entry */
      if (size == 0)
        ERREXIT(state->cinfo, JERR_HUFF_MISSING_CODE);

      /* mask off any extra bits in code */
      put_buffer = ((INT32) code) & ((((INT32) 1) << size) - 1);

      /* new number of bits in buffer */
      put_bits = size + state->cur.put_bits;

      put_buffer <<= 24 - put_bits; /* align incoming bits */

      /* and merge with old buffer contents */
      put_buffer |= state->cur.put_buffer;

      while (put_bits >= 8) {
        int c = (int) ((put_buffer >> 16) & 0xFF);

        emit_byte_s(state, c, return FALSE);
        if (c == 0xFF) {		/* need to stuff a zero byte? */
          emit_byte_s(state, 0, return FALSE);
        }
        put_buffer <<= 8;
        put_bits -= 8;
      }

      state->cur.put_buffer = put_buffer; /* update state variables */
      state->cur.put_bits = put_bits;

      return TRUE;
    }

    INLINE
    LOCAL(void)
    emit_bits_e (huff_entropy_ptr entropy, unsigned int code, int size)
    /* Emit some bits, unless we are in gather mode */
    {
      /* This routine is heavily used, so it's worth coding tightly. */
      register INT32 put_buffer;
      register int put_bits;

      /* if size is 0, caller used an invalid Huffman table entry */
      if (size == 0)
        ERREXIT(entropy->cinfo, JERR_HUFF_MISSING_CODE);

      if (entropy->gather_statistics)
        return;			/* do nothing if we're only getting stats */

      /* mask off any extra bits in code */
      put_buffer = ((INT32) code) & ((((INT32) 1) << size) - 1);

      /* new number of bits in buffer */
      put_bits = size + entropy->saved.put_bits;

      put_buffer <<= 24 - put_bits; /* align incoming bits */

      /* and merge with old buffer contents */
      put_buffer |= entropy->saved.put_buffer;

      while (put_bits >= 8) {
        int c = (int) ((put_buffer >> 16) & 0xFF);

        emit_byte_e(entropy, c);
        if (c == 0xFF) {		/* need to stuff a zero byte? */
          emit_byte_e(entropy, 0);
        }
        put_buffer <<= 8;
        put_bits -= 8;
      }

      entropy->saved.put_buffer = put_buffer; /* update variables */
      entropy->saved.put_bits = put_bits;
    }

    LOCAL(boolean)
    flush_bits_s (working_state * state)
    {
      if (! emit_bits_s(state, 0x7F, 7)) /* fill any partial byte with ones */
        return FALSE;
      state->cur.put_buffer = 0;	     /* and reset bit-buffer to empty */
      state->cur.put_bits = 0;
      return TRUE;
    }

    LOCAL(void)
    flush_bits_e (huff_entropy_ptr entropy)
    {
      emit_bits_e(entropy, 0x7F, 7); /* fill any partial byte with ones */
      entropy->saved.put_buffer = 0; /* and reset bit-buffer to empty */
      entropy->saved.put_bits = 0;
    }

    /*
     * Emit (or just count) a Huffman symbol.
     */

    INLINE
    LOCAL(void)
    emit_dc_symbol (huff_entropy_ptr entropy, int tbl_no, int symbol)
    {
      if (entropy->gather_statistics)
        entropy->dc_count_ptrs[tbl_no][symbol]++;
      else {
        c_derived_tbl * tbl = entropy->dc_derived_tbls[tbl_no];
        emit_bits_e(entropy, tbl->ehufco[symbol], tbl->ehufsi[symbol]);
      }
    }

    INLINE
    LOCAL(void)
    emit_ac_symbol (huff_entropy_ptr entropy, int tbl_no, int symbol)
    {
      if (entropy->gather_statistics)
        entropy->ac_count_ptrs[tbl_no][symbol]++;
      else {
        c_derived_tbl * tbl = entropy->ac_derived_tbls[tbl_no];
        emit_bits_e(entropy, tbl->ehufco[symbol], tbl->ehufsi[symbol]);
      }
    }

    /*
     * Emit bits from a correction bit buffer.
     */

    LOCAL(void)
    emit_buffered_bits (huff_entropy_ptr entropy, char * bufstart,
    		    unsigned int nbits)
    {
      if (entropy->gather_statistics)
        return;			/* no real work */

      while (nbits > 0) {
        emit_bits_e(entropy, (unsigned int) (*bufstart), 1);
        bufstart++;
        nbits--;
      }
    }

    /*
     * Emit any pending EOBRUN symbol.
     */

    LOCAL(void)
    emit_eobrun (huff_entropy_ptr entropy)
    {
      register int temp, nbits;

      if (entropy->EOBRUN > 0) {	/* if there is any pending EOBRUN */
        temp = entropy->EOBRUN;
        nbits = 0;
        while ((temp >>= 1))
          nbits++;
        /* safety check: shouldn't happen given limited correction-bit buffer */
        if (nbits > 14)
          ERREXIT(entropy->cinfo, JERR_HUFF_MISSING_CODE);

        emit_ac_symbol(entropy, entropy->ac_tbl_no, nbits << 4);
        if (nbits)
          emit_bits_e(entropy, entropy->EOBRUN, nbits);

        entropy->EOBRUN = 0;

        /* Emit any buffered correction bits */
        emit_buffered_bits(entropy, entropy->bit_buffer, entropy->BE);
        entropy->BE = 0;
      }
    }

    /*
     * Emit a restart marker & resynchronize predictions.
     */

    LOCAL(boolean)
    emit_restart_s (working_state * state, int restart_num)
    {
      int ci;

      if (! flush_bits_s(state))
        return FALSE;

      emit_byte_s(state, 0xFF, return FALSE);
      emit_byte_s(state, JPEG_RST0 + restart_num, return FALSE);

      /* Re-initialize DC predictions to 0 */
      for (ci = 0; ci < state->cinfo->comps_in_scan; ci++)
        state->cur.last_dc_val[ci] = 0;

      /* The restart counter is not updated until we successfully write the MCU. */

      return TRUE;
    }

    LOCAL(void)
    emit_restart_e (huff_entropy_ptr entropy, int restart_num)
    {
      int ci;

      emit_eobrun(entropy);

      if (! entropy->gather_statistics) {
        flush_bits_e(entropy);
        emit_byte_e(entropy, 0xFF);
        emit_byte_e(entropy, JPEG_RST0 + restart_num);
      }

      if (entropy->cinfo->Ss == 0) {
        /* Re-initialize DC predictions to 0 */
        for (ci = 0; ci < entropy->cinfo->comps_in_scan; ci++)
          entropy->saved.last_dc_val[ci] = 0;
      } else {
        /* Re-initialize all AC-related fields to 0 */
        entropy->EOBRUN = 0;
        entropy->BE = 0;
      }
    }

    /*
     * MCU encoding for DC initial scan (either spectral selection,
     * or first pass of successive approximation).
     */

    METHODDEF(boolean)
    encode_mcu_DC_first (j_compress_ptr cinfo, JBLOCKARRAY MCU_data)
    {
      huff_entropy_ptr entropy = (huff_entropy_ptr) cinfo->entropy;
      register int temp, temp2;
      register int nbits;
      int blkn, ci, tbl;
      ISHIFT_TEMPS

      entropy->next_output_byte = cinfo->dest->next_output_byte;
      entropy->free_in_buffer = cinfo->dest->free_in_buffer;

      /* Emit restart marker if needed */
      if (cinfo->restart_interval)
        if (entropy->restarts_to_go == 0)
          emit_restart_e(entropy, entropy->next_restart_num);

      /* Encode the MCU data blocks */
      for (blkn = 0; blkn < cinfo->blocks_in_MCU; blkn++) {
        ci = cinfo->MCU_membership[blkn];
        tbl = cinfo->cur_comp_info[ci]->dc_tbl_no;

        /* Compute the DC value after the required point transform by Al.
         * This is simply an arithmetic right shift.
         */
        temp = IRIGHT_SHIFT((int) (MCU_data[blkn][0][0]), cinfo->Al);

        /* DC differences are figured on the point-transformed values. */
        temp2 = temp - entropy->saved.last_dc_val[ci];
        entropy->saved.last_dc_val[ci] = temp;

        /* Encode the DC coefficient difference per section G.1.2.1 */
        temp = temp2;
        if (temp < 0) {
          temp = -temp;		/* temp is abs value of input */
          /* For a negative input, want temp2 = bitwise complement of abs(input) */
          /* This code assumes we are on a two's complement machine */
          temp2--;
        }

        /* Find the number of bits needed for the magnitude of the coefficient */
        nbits = 0;
        while (temp) {
          nbits++;
          temp >>= 1;
        }
        /* Check for out-of-range coefficient values.
         * Since we're encoding a difference, the range limit is twice as much.
         */
        if (nbits > MAX_COEF_BITS+1)
          ERREXIT(cinfo, JERR_BAD_DCT_COEF);

        /* Count/emit the Huffman-coded symbol for the number of bits */
        emit_dc_symbol(entropy, tbl, nbits);

        /* Emit that number of bits of the value, if positive, */
        /* or the complement of its magnitude, if negative. */
        if (nbits)			/* emit_bits rejects calls with size 0 */
          emit_bits_e(entropy, (unsigned int) temp2, nbits);
      }

      cinfo->dest->next_output_byte = entropy->next_output_byte;
      cinfo->dest->free_in_buffer = entropy->free_in_buffer;

      /* Update restart-interval state too */
      if (cinfo->restart_interval) {
        if (entropy->restarts_to_go == 0) {
          entropy->restarts_to_go = cinfo->restart_interval;
          entropy->next_restart_num++;
          entropy->next_restart_num &= 7;
        }
        entropy->restarts_to_go--;
      }

      return TRUE;
    }

    /*
     * MCU encoding for AC initial scan (either spectral selection,
     * or first pass of successive approximation).
     */

    METHODDEF(boolean)
    encode_mcu_AC_first (j_compress_ptr cinfo, JBLOCKARRAY MCU_data)
    {
      huff_entropy_ptr entropy = (huff_entropy_ptr) cinfo->entropy;
      const int * natural_order;
      JBLOCKROW block;
      register int temp, temp2;
      register int nbits;
      register int r, k;
      int Se, Al;

      entropy->next_output_byte = cinfo->dest->next_output_byte;
      entropy->free_in_buffer = cinfo->dest->free_in_buffer;

      /* Emit restart marker if needed */
      if (cinfo->restart_interval)
        if (entropy->restarts_to_go == 0)
          emit_restart_e(entropy, entropy->next_restart_num);

      Se = cinfo->Se;
      Al = cinfo->Al;
      natural_order = cinfo->natural_order;

      /* Encode the MCU data block */
      block = MCU_data[0];

      /* Encode the AC coefficients per section G.1.2.2, fig. G.3 */

      r = 0;			/* r = run length of zeros */

      for (k = cinfo->Ss; k <= Se; k++) {
        if ((temp = (*block)[natural_order[k]]) == 0) {
          r++;
          continue;
        }
        /* We must apply the point transform by Al.  For AC coefficients this
         * is an integer division with rounding towards 0.  To do this portably
         * in C, we shift after obtaining the absolute value; so the code is
         * interwoven with finding the abs value (temp) and output bits (temp2).
         */
        if (temp < 0) {
          temp = -temp;		/* temp is abs value of input */
          temp >>= Al;		/* apply the point transform */
          /* For a negative coef, want temp2 = bitwise complement of abs(coef) */
          temp2 = ~temp;
        } else {
          temp >>= Al;		/* apply the point transform */
          temp2 = temp;
        }
        /* Watch out for case that nonzero coef is zero after point transform */
        if (temp == 0) {
          r++;
          continue;
        }

        /* Emit any pending EOBRUN */
        if (entropy->EOBRUN > 0)
          emit_eobrun(entropy);
        /* if run length > 15, must emit special run-length-16 codes (0xF0) */
        while (r > 15) {
          emit_ac_symbol(entropy, entropy->ac_tbl_no, 0xF0);
          r -= 16;
        }

        /* Find the number of bits needed for the magnitude of the coefficient */
        nbits = 1;			/* there must be at least one 1 bit */
        while ((temp >>= 1))
          nbits++;
        /* Check for out-of-range coefficient values */
        if (nbits > MAX_COEF_BITS)
          ERREXIT(cinfo, JERR_BAD_DCT_COEF);

        /* Count/emit Huffman symbol for run length / number of bits */
        emit_ac_symbol(entropy, entropy->ac_tbl_no, (r << 4) + nbits);

        /* Emit that number of bits of the value, if positive, */
        /* or the complement of its magnitude, if negative. */
        emit_bits_e(entropy, (unsigned int) temp2, nbits);

        r = 0;			/* reset zero run length */
      }

      if (r > 0) {			/* If there are trailing zeroes, */
        entropy->EOBRUN++;		/* count an EOB */
        if (entropy->EOBRUN == 0x7FFF)
          emit_eobrun(entropy);	/* force it out to avoid overflow */
      }

      cinfo->dest->next_output_byte = entropy->next_output_byte;
      cinfo->dest->free_in_buffer = entropy->free_in_buffer;

      /* Update restart-interval state too */
      if (cinfo->restart_interval) {
        if (entropy->restarts_to_go == 0) {
          entropy->restarts_to_go = cinfo->restart_interval;
          entropy->next_restart_num++;
          entropy->next_restart_num &= 7;
        }
        entropy->restarts_to_go--;
      }

      return TRUE;
    }

    /*
     * MCU encoding for DC successive approximation refinement scan.
     * Note: we assume such scans can be multi-component,
     * although the spec is not very clear on the point.
     */

    METHODDEF(boolean)
    encode_mcu_DC_refine (j_compress_ptr cinfo, JBLOCKARRAY MCU_data)
    {
      huff_entropy_ptr entropy = (huff_entropy_ptr) cinfo->entropy;
      int Al, blkn;

      entropy->next_output_byte = cinfo->dest->next_output_byte;
      entropy->free_in_buffer = cinfo->dest->free_in_buffer;

      /* Emit restart marker if needed */
      if (cinfo->restart_interval)
        if (entropy->restarts_to_go == 0)
          emit_restart_e(entropy, entropy->next_restart_num);

      Al = cinfo->Al;

      /* Encode the MCU data blocks */
      for (blkn = 0; blkn < cinfo->blocks_in_MCU; blkn++) {
        /* We simply emit the Al'th bit of the DC coefficient value. */
        emit_bits_e(entropy, (unsigned int) (MCU_data[blkn][0][0] >> Al), 1);
      }

      cinfo->dest->next_output_byte = entropy->next_output_byte;
      cinfo->dest->free_in_buffer = entropy->free_in_buffer;

      /* Update restart-interval state too */
      if (cinfo->restart_interval) {
        if (entropy->restarts_to_go == 0) {
          entropy->restarts_to_go = cinfo->restart_interval;
          entropy->next_restart_num++;
          entropy->next_restart_num &= 7;
        }
        entropy->restarts_to_go--;
      }

      return TRUE;
    }

    /*
     * MCU encoding for AC successive approximation refinement scan.
     */

    METHODDEF(boolean)
    encode_mcu_AC_refine (j_compress_ptr cinfo, JBLOCKARRAY MCU_data)
    {
      huff_entropy_ptr entropy = (huff_entropy_ptr) cinfo->entropy;
      const int * natural_order;
      JBLOCKROW block;
      register int temp;
      register int r, k;
      int Se, Al;
      int EOB;
      char *BR_buffer;
      unsigned int BR;
      int absvalues[DCTSIZE2];

      entropy->next_output_byte = cinfo->dest->next_output_byte;
      entropy->free_in_buffer = cinfo->dest->free_in_buffer;

      /* Emit restart marker if needed */
      if (cinfo->restart_interval)
        if (entropy->restarts_to_go == 0)
          emit_restart_e(entropy, entropy->next_restart_num);

      Se = cinfo->Se;
      Al = cinfo->Al;
      natural_order = cinfo->natural_order;

      /* Encode the MCU data block */
      block = MCU_data[0];

      /* It is convenient to make a pre-pass to determine the transformed
       * coefficients' absolute values and the EOB position.
       */
      EOB = 0;
      for (k = cinfo->Ss; k <= Se; k++) {
        temp = (*block)[natural_order[k]];
        /* We must apply the point transform by Al.  For AC coefficients this
         * is an integer division with rounding towards 0.  To do this portably
         * in C, we shift after obtaining the absolute value.
         */
        if (temp < 0)
          temp = -temp;		/* temp is abs value of input */
        temp >>= Al;		/* apply the point transform */
        absvalues[k] = temp;	/* save abs value for main pass */
        if (temp == 1)
          EOB = k;			/* EOB = index of last newly-nonzero coef */
      }

      /* Encode the AC coefficients per section G.1.2.3, fig. G.7 */

      r = 0;			/* r = run length of zeros */
      BR = 0;			/* BR = count of buffered bits added now */
      BR_buffer = entropy->bit_buffer + entropy->BE; /* Append bits to buffer */

      for (k = cinfo->Ss; k <= Se; k++) {
        if ((temp = absvalues[k]) == 0) {
          r++;
          continue;
        }

        /* Emit any required ZRLs, but not if they can be folded into EOB */
        while (r > 15 && k <= EOB) {
          /* emit any pending EOBRUN and the BE correction bits */
          emit_eobrun(entropy);
          /* Emit ZRL */
          emit_ac_symbol(entropy, entropy->ac_tbl_no, 0xF0);
          r -= 16;
          /* Emit buffered correction bits that must be associated with ZRL */
          emit_buffered_bits(entropy, BR_buffer, BR);
          BR_buffer = entropy->bit_buffer; /* BE bits are gone now */
          BR = 0;
        }

        /* If the coef was previously nonzero, it only needs a correction bit.
         * NOTE: a straight translation of the spec's figure G.7 would suggest
         * that we also need to test r > 15.  But if r > 15, we can only get here
         * if k > EOB, which implies that this coefficient is not 1.
         */
        if (temp > 1) {
          /* The correction bit is the next bit of the absolute value. */
          BR_buffer[BR++] = (char) (temp & 1);
          continue;
        }

        /* Emit any pending EOBRUN and the BE correction bits */
        emit_eobrun(entropy);

        /* Count/emit Huffman symbol for run length / number of bits */
        emit_ac_symbol(entropy, entropy->ac_tbl_no, (r << 4) + 1);

        /* Emit output bit for newly-nonzero coef */
        temp = ((*block)[natural_order[k]] < 0) ? 0 : 1;
        emit_bits_e(entropy, (unsigned int) temp, 1);

        /* Emit buffered correction bits that must be associated with this code */
        emit_buffered_bits(entropy, BR_buffer, BR);
        BR_buffer = entropy->bit_buffer; /* BE bits are gone now */
        BR = 0;
        r = 0;			/* reset zero run length */
      }

      if (r > 0 || BR > 0) {	/* If there are trailing zeroes, */
        entropy->EOBRUN++;		/* count an EOB */
        entropy->BE += BR;		/* concat my correction bits to older ones */
        /* We force out the EOB if we risk either:
         * 1. overflow of the EOB counter;
         * 2. overflow of the correction bit buffer during the next MCU.
         */
        if (entropy->EOBRUN == 0x7FFF || entropy->BE > (MAX_CORR_BITS-DCTSIZE2+1))
          emit_eobrun(entropy);
      }

      cinfo->dest->next_output_byte = entropy->next_output_byte;
      cinfo->dest->free_in_buffer = entropy->free_in_buffer;

      /* Update restart-interval state too */
      if (cinfo->restart_interval) {
        if (entropy->restarts_to_go == 0) {
          entropy->restarts_to_go = cinfo->restart_interval;
          entropy->next_restart_num++;
          entropy->next_restart_num &= 7;
        }
        entropy->restarts_to_go--;
      }

      return TRUE;
    }

    /* Encode a single block's worth of coefficients */

    LOCAL(boolean)
    encode_one_block (working_state * state, JCOEFPTR block, int last_dc_val,
    		  c_derived_tbl *dctbl, c_derived_tbl *actbl)
    {
      register int temp, temp2;
      register int nbits;
      register int r, k;
      int Se = state->cinfo->lim_Se;
      const int * natural_order = state->cinfo->natural_order;

      /* Encode the DC coefficient difference per section F.1.2.1 */

      temp = temp2 = block[0] - last_dc_val;

      if (temp < 0) {
        temp = -temp;		/* temp is abs value of input */
        /* For a negative input, want temp2 = bitwise complement of abs(input) */
        /* This code assumes we are on a two's complement machine */
        temp2--;
      }

      /* Find the number of bits needed for the magnitude of the coefficient */
      nbits = 0;
      while (temp) {
        nbits++;
        temp >>= 1;
      }
      /* Check for out-of-range coefficient values.
       * Since we're encoding a difference, the range limit is twice as much.
       */
      if (nbits > MAX_COEF_BITS+1)
        ERREXIT(state->cinfo, JERR_BAD_DCT_COEF);

      /* Emit the Huffman-coded symbol for the number of bits */
      if (! emit_bits_s(state, dctbl->ehufco[nbits], dctbl->ehufsi[nbits]))
        return FALSE;

      /* Emit that number of bits of the value, if positive, */
      /* or the complement of its magnitude, if negative. */
      if (nbits)			/* emit_bits rejects calls with size 0 */
        if (! emit_bits_s(state, (unsigned int) temp2, nbits))
          return FALSE;

      /* Encode the AC coefficients per section F.1.2.2 */

      r = 0;			/* r = run length of zeros */

      for (k = 1; k <= Se; k++) {
        if ((temp2 = block[natural_order[k]]) == 0) {
          r++;
        } else {
          /* if run length > 15, must emit special run-length-16 codes (0xF0) */
          while (r > 15) {
    	if (! emit_bits_s(state, actbl->ehufco[0xF0], actbl->ehufsi[0xF0]))
    	  return FALSE;
    	r -= 16;
          }

          temp = temp2;
          if (temp < 0) {
    	temp = -temp;		/* temp is abs value of input */
    	/* This code assumes we are on a two's complement machine */
    	temp2--;
          }

          /* Find the number of bits needed for the magnitude of the coefficient */
          nbits = 1;		/* there must be at least one 1 bit */
          while ((temp >>= 1))
    	nbits++;
          /* Check for out-of-range coefficient values */
          if (nbits > MAX_COEF_BITS)
    	ERREXIT(state->cinfo, JERR_BAD_DCT_COEF);

          /* Emit Huffman symbol for run length / number of bits */
          temp = (r << 4) + nbits;
          if (! emit_bits_s(state, actbl->ehufco[temp], actbl->ehufsi[temp]))
    	return FALSE;

          /* Emit that number of bits of the value, if positive, */
          /* or the complement of its magnitude, if negative. */
          if (! emit_bits_s(state, (unsigned int) temp2, nbits))
    	return FALSE;

          r = 0;
        }
      }

      /* If the last coef(s) were zero, emit an end-of-block code */
      if (r > 0)
        if (! emit_bits_s(state, actbl->ehufco[0], actbl->ehufsi[0]))
          return FALSE;

      return TRUE;
    }

    /*
     * Encode and output one MCU's worth of Huffman-compressed coefficients.
     */

    METHODDEF(boolean)
    encode_mcu_huff (j_compress_ptr cinfo, JBLOCKARRAY MCU_data)
    {
      huff_entropy_ptr entropy = (huff_entropy_ptr) cinfo->entropy;
      working_state state;
      int blkn, ci;
      jpeg_component_info * compptr;

      /* Load up working state */
      state.next_output_byte = cinfo->dest->next_output_byte;
      state.free_in_buffer = cinfo->dest->free_in_buffer;
      ASSIGN_STATE(state.cur, entropy->saved);
      state.cinfo = cinfo;

      /* Emit restart marker if needed */
      if (cinfo->restart_interval) {
        if (entropy->restarts_to_go == 0)
          if (! emit_restart_s(&state, entropy->next_restart_num))
    	return FALSE;
      }

      /* Encode the MCU data blocks */
      for (blkn = 0; blkn < cinfo->blocks_in_MCU; blkn++) {
        ci = cinfo->MCU_membership[blkn];
        compptr = cinfo->cur_comp_info[ci];
        if (! encode_one_block(&state,
    			   MCU_data[blkn][0], state.cur.last_dc_val[ci],
    			   entropy->dc_derived_tbls[compptr->dc_tbl_no],
    			   entropy->ac_derived_tbls[compptr->ac_tbl_no]))
          return FALSE;
        /* Update last_dc_val */
        state.cur.last_dc_val[ci] = MCU_data[blkn][0][0];
      }

      /* Completed MCU, so update state */
      cinfo->dest->next_output_byte = state.next_output_byte;
      cinfo->dest->free_in_buffer = state.free_in_buffer;
      ASSIGN_STATE(entropy->saved, state.cur);

      /* Update restart-interval state too */
      if (cinfo->restart_interval) {
        if (entropy->restarts_to_go == 0) {
          entropy->restarts_to_go = cinfo->restart_interval;
          entropy->next_restart_num++;
          entropy->next_restart_num &= 7;
        }
        entropy->restarts_to_go--;
      }

      return TRUE;
    }

    /*
     * Finish up at the end of a Huffman-compressed scan.
     */

    METHODDEF(void)
    finish_pass_huff (j_compress_ptr cinfo)
    {
      huff_entropy_ptr entropy = (huff_entropy_ptr) cinfo->entropy;
      working_state state;

      if (cinfo->progressive_mode) {
        entropy->next_output_byte = cinfo->dest->next_output_byte;
        entropy->free_in_buffer = cinfo->dest->free_in_buffer;

        /* Flush out any buffered data */
        emit_eobrun(entropy);
        flush_bits_e(entropy);

        cinfo->dest->next_output_byte = entropy->next_output_byte;
        cinfo->dest->free_in_buffer = entropy->free_in_buffer;
      } else {
        /* Load up working state ... flush_bits needs it */
        state.next_output_byte = cinfo->dest->next_output_byte;
        state.free_in_buffer = cinfo->dest->free_in_buffer;
        ASSIGN_STATE(state.cur, entropy->saved);
        state.cinfo = cinfo;

        /* Flush out the last data */
        if (! flush_bits_s(&state))
          ERREXIT(cinfo, JERR_CANT_SUSPEND);

        /* Update state */
        cinfo->dest->next_output_byte = state.next_output_byte;
        cinfo->dest->free_in_buffer = state.free_in_buffer;
        ASSIGN_STATE(entropy->saved, state.cur);
      }
    }

    /*
     * Huffman coding optimization.
     *
     * We first scan the supplied data and count the number of uses of each symbol
     * that is to be Huffman-coded. (This process MUST agree with the code above.)
     * Then we build a Huffman coding tree for the observed counts.
     * Symbols which are not needed at all for the particular image are not
     * assigned any code, which saves space in the DHT marker as well as in
     * the compressed data.
     */

    /* Process a single block's worth of coefficients */

    LOCAL(void)
    htest_one_block (j_compress_ptr cinfo, JCOEFPTR block, int last_dc_val,
    		 long dc_counts[], long ac_counts[])
    {
      register int temp;
      register int nbits;
      register int r, k;
      int Se = cinfo->lim_Se;
      const int * natural_order = cinfo->natural_order;

      /* Encode the DC coefficient difference per section F.1.2.1 */

      temp = block[0] - last_dc_val;
      if (temp < 0)
        temp = -temp;

      /* Find the number of bits needed for the magnitude of the coefficient */
      nbits = 0;
      while (temp) {
        nbits++;
        temp >>= 1;
      }
      /* Check for out-of-range coefficient values.
       * Since we're encoding a difference, the range limit is twice as much.
       */
      if (nbits > MAX_COEF_BITS+1)
        ERREXIT(cinfo, JERR_BAD_DCT_COEF);

      /* Count the Huffman symbol for the number of bits */
      dc_counts[nbits]++;

      /* Encode the AC coefficients per section F.1.2.2 */

      r = 0;			/* r = run length of zeros */

      for (k = 1; k <= Se; k++) {
        if ((temp = block[natural_order[k]]) == 0) {
          r++;
        } else {
          /* if run length > 15, must emit special run-length-16 codes (0xF0) */
          while (r > 15) {
    	ac_counts[0xF0]++;
    	r -= 16;
          }

          /* Find the number of bits needed for the magnitude of the coefficient */
          if (temp < 0)
    	temp = -temp;

          /* Find the number of bits needed for the magnitude of the coefficient */
          nbits = 1;		/* there must be at least one 1 bit */
          while ((temp >>= 1))
    	nbits++;
          /* Check for out-of-range coefficient values */
          if (nbits > MAX_COEF_BITS)
    	ERREXIT(cinfo, JERR_BAD_DCT_COEF);

          /* Count Huffman symbol for run length / number of bits */
          ac_counts[(r << 4) + nbits]++;

          r = 0;
        }
      }

      /* If the last coef(s) were zero, emit an end-of-block code */
      if (r > 0)
        ac_counts[0]++;
    }

    /*
     * Trial-encode one MCU's worth of Huffman-compressed coefficients.
     * No data is actually output, so no suspension return is possible.
     */

    METHODDEF(boolean)
    encode_mcu_gather (j_compress_ptr cinfo, JBLOCKARRAY MCU_data)
    {
      huff_entropy_ptr entropy = (huff_entropy_ptr) cinfo->entropy;
      int blkn, ci;
      jpeg_component_info * compptr;

      /* Take care of restart intervals if needed */
      if (cinfo->restart_interval) {
        if (entropy->restarts_to_go == 0) {
          /* Re-initialize DC predictions to 0 */
          for (ci = 0; ci < cinfo->comps_in_scan; ci++)
    	entropy->saved.last_dc_val[ci] = 0;
          /* Update restart state */
          entropy->restarts_to_go = cinfo->restart_interval;
        }
        entropy->restarts_to_go--;
      }

      for (blkn = 0; blkn < cinfo->blocks_in_MCU; blkn++) {
        ci = cinfo->MCU_membership[blkn];
        compptr = cinfo->cur_comp_info[ci];
        htest_one_block(cinfo, MCU_data[blkn][0], entropy->saved.last_dc_val[ci],
    		    entropy->dc_count_ptrs[compptr->dc_tbl_no],
    		    entropy->ac_count_ptrs[compptr->ac_tbl_no]);
        entropy->saved.last_dc_val[ci] = MCU_data[blkn][0][0];
      }

      return TRUE;
    }

    /*
     * Generate the best Huffman code table for the given counts, fill htbl.
     *
     * The JPEG standard requires that no symbol be assigned a codeword of all
     * one bits (so that padding bits added at the end of a compressed segment
     * can't look like a valid code).  Because of the canonical ordering of
     * codewords, this just means that there must be an unused slot in the
     * longest codeword length category.  Section K.2 of the JPEG spec suggests
     * reserving such a slot by pretending that symbol 256 is a valid symbol
     * with count 1.  In theory that's not optimal; giving it count zero but
     * including it in the symbol set anyway should give a better Huffman code.
     * But the theoretically better code actually seems to come out worse in
     * practice, because it produces more all-ones bytes (which incur stuffed
     * zero bytes in the final file).  In any case the difference is tiny.
     *
     * The JPEG standard requires Huffman codes to be no more than 16 bits long.
     * If some symbols have a very small but nonzero probability, the Huffman tree
     * must be adjusted to meet the code length restriction.  We currently use
     * the adjustment method suggested in JPEG section K.2.  This method is *not*
     * optimal; it may not choose the best possible limited-length code.  But
     * typically only very-low-frequency symbols will be given less-than-optimal
     * lengths, so the code is almost optimal.  Experimental comparisons against
     * an optimal limited-length-code algorithm indicate that the difference is
     * microscopic --- usually less than a hundredth of a percent of total size.
     * So the extra complexity of an optimal algorithm doesn't seem worthwhile.
     */

    LOCAL(void)
    jpeg_gen_optimal_table (j_compress_ptr cinfo, JHUFF_TBL * htbl, long freq[])
    {
    #define MAX_CLEN 32		/* assumed maximum initial code length */
      UINT8 bits[MAX_CLEN+1];	/* bits[k] = # of symbols with code length k */
      int codesize[257];		/* codesize[k] = code length of symbol k */
      int others[257];		/* next symbol in current branch of tree */
      int c1, c2, i, j;
      UINT8 *p;
      long v;

      freq[256] = 1;		/* make sure 256 has a nonzero count */
      /* Including the pseudo-symbol 256 in the Huffman procedure guarantees
       * that no real symbol is given code-value of all ones, because 256
       * will be placed last in the largest codeword category.
       * In the symbol list build procedure this element serves as sentinel
       * for the zero run loop.
       */

    #ifndef DONT_USE_FANCY_HUFF_OPT

      /* Build list of symbols sorted in order of descending frequency */
      /* This approach has several benefits (thank to John Korejwa for the idea):
       *     1.
       * If a codelength category is split during the length limiting procedure
       * below, the feature that more frequent symbols are assigned shorter
       * codewords remains valid for the adjusted code.
       *     2.
       * To reduce consecutive ones in a Huffman data stream (thus reducing the
       * number of stuff bytes in JPEG) it is preferable to follow 0 branches
       * (and avoid 1 branches) as much as possible.  This is easily done by
       * assigning symbols to leaves of the Huffman tree in order of decreasing
       * frequency, with no secondary sort based on codelengths.
       *     3.
       * The symbol list can be built independently from the assignment of code
       * lengths by the Huffman procedure below.
       * Note: The symbol list build procedure must be performed first, because
       * the Huffman procedure assigning the codelengths clobbers the frequency
       * counts!
       */

      /* Here we use the others array as a linked list of nonzero frequencies
       * to be sorted.  Already sorted elements are removed from the list.
       */

      /* Building list */

      /* This item does not correspond to a valid symbol frequency and is used
       * as starting index.
       */
      j = 256;

      for (i = 0;; i++) {
        if (freq[i] == 0)		/* skip zero frequencies */
          continue;
        if (i > 255)
          break;
        others[j] = i;		/* this symbol value */
        j = i;			/* previous symbol value */
      }
      others[j] = -1;		/* mark end of list */

      /* Sorting list */

      p = htbl->huffval;
      while ((c1 = others[256]) >= 0) {
        v = freq[c1];
        i = c1;			/* first symbol value */
        j = 256;			/* pseudo symbol value for starting index */
        while ((c2 = others[c1]) >= 0) {
          if (freq[c2] > v) {
    	v = freq[c2];
    	i = c2;			/* this symbol value */
    	j = c1;			/* previous symbol value */
          }
          c1 = c2;
        }
        others[j] = others[i];	/* remove this symbol i from list */
        *p++ = (UINT8) i;
      }

    #endif /* DONT_USE_FANCY_HUFF_OPT */

      /* This algorithm is explained in section K.2 of the JPEG standard */

      MEMZERO(bits, SIZEOF(bits));
      MEMZERO(codesize, SIZEOF(codesize));
      for (i = 0; i < 257; i++)
        others[i] = -1;		/* init links to empty */

      /* Huffman's basic algorithm to assign optimal code lengths to symbols */

      for (;;) {
        /* Find the smallest nonzero frequency, set c1 = its symbol */
        /* In case of ties, take the larger symbol number */
        c1 = -1;
        v = 1000000000L;
        for (i = 0; i <= 256; i++) {
          if (freq[i] && freq[i] <= v) {
    	v = freq[i];
    	c1 = i;
          }
        }

        /* Find the next smallest nonzero frequency, set c2 = its symbol */
        /* In case of ties, take the larger symbol number */
        c2 = -1;
        v = 1000000000L;
        for (i = 0; i <= 256; i++) {
          if (freq[i] && freq[i] <= v && i != c1) {
    	v = freq[i];
    	c2 = i;
          }
        }

        /* Done if we've merged everything into one frequency */
        if (c2 < 0)
          break;

        /* Else merge the two counts/trees */
        freq[c1] += freq[c2];
        freq[c2] = 0;

        /* Increment the codesize of everything in c1's tree branch */
        codesize[c1]++;
        while (others[c1] >= 0) {
          c1 = others[c1];
          codesize[c1]++;
        }

        others[c1] = c2;		/* chain c2 onto c1's tree branch */

        /* Increment the codesize of everything in c2's tree branch */
        codesize[c2]++;
        while (others[c2] >= 0) {
          c2 = others[c2];
          codesize[c2]++;
        }
      }

      /* Now count the number of symbols of each code length */
      for (i = 0; i <= 256; i++) {
        if (codesize[i]) {
          /* The JPEG standard seems to think that this can't happen, */
          /* but I'm paranoid... */
          if (codesize[i] > MAX_CLEN)
    	ERREXIT(cinfo, JERR_HUFF_CLEN_OUTOFBOUNDS);

          bits[codesize[i]]++;
        }
      }

      /* JPEG doesn't allow symbols with code lengths over 16 bits, so if the pure
       * Huffman procedure assigned any such lengths, we must adjust the coding.
       * Here is what the JPEG spec says about how this next bit works:
       * Since symbols are paired for the longest Huffman code, the symbols are
       * removed from this length category two at a time.  The prefix for the pair
       * (which is one bit shorter) is allocated to one of the pair; then,
       * skipping the BITS entry for that prefix length, a code word from the next
       * shortest nonzero BITS entry is converted into a prefix for two code words
       * one bit longer.
       */

      for (i = MAX_CLEN; i > 16; i--) {
        while (bits[i] > 0) {
          j = i - 2;		/* find length of new prefix to be used */
          while (bits[j] == 0) {
    	if (j == 0)
    	  ERREXIT(cinfo, JERR_HUFF_CLEN_OUTOFBOUNDS);
    	j--;
          }

          bits[i] -= 2;		/* remove two symbols */
          bits[i-1]++;		/* one goes in this length */
          bits[j+1] += 2;		/* two new symbols in this length */
          bits[j]--;		/* symbol of this length is now a prefix */
        }
      }

      /* Remove the count for the pseudo-symbol 256 from the largest codelength */
      while (bits[i] == 0)		/* find largest codelength still in use */
        i--;
      bits[i]--;

      /* Return final symbol counts (only for lengths 0..16) */
      MEMCOPY(htbl->bits, bits, SIZEOF(htbl->bits));

    #ifdef DONT_USE_FANCY_HUFF_OPT

      /* Return a list of the symbols sorted by code length */
      /* Note: Due to the codelength changes made above, it can happen
       * that more frequent symbols are assigned longer codewords.
       */
      p = htbl->huffval;
      for (i = 1; i <= MAX_CLEN; i++) {
        for (j = 0; j <= 255; j++) {
          if (codesize[j] == i) {
    	*p++ = (UINT8) j;
          }
        }
      }

    #endif /* DONT_USE_FANCY_HUFF_OPT */

      /* Set sent_table FALSE so updated table will be written to JPEG file. */
      htbl->sent_table = FALSE;
    }

    /*
     * Finish up a statistics-gathering pass and create the new Huffman tables.
     */

    METHODDEF(void)
    finish_pass_gather (j_compress_ptr cinfo)
    {
      huff_entropy_ptr entropy = (huff_entropy_ptr) cinfo->entropy;
      int ci, tbl;
      jpeg_component_info * compptr;
      JHUFF_TBL **htblptr;
      boolean did_dc[NUM_HUFF_TBLS];
      boolean did_ac[NUM_HUFF_TBLS];

      if (cinfo->progressive_mode)
        /* Flush out buffered data (all we care about is counting the EOB symbol) */
        emit_eobrun(entropy);

      /* It's important not to apply jpeg_gen_optimal_table more than once
       * per table, because it clobbers the input frequency counts!
       */
      MEMZERO(did_dc, SIZEOF(did_dc));
      MEMZERO(did_ac, SIZEOF(did_ac));

      for (ci = 0; ci < cinfo->comps_in_scan; ci++) {
        compptr = cinfo->cur_comp_info[ci];
        /* DC needs no table for refinement scan */
        if (cinfo->Ss == 0 && cinfo->Ah == 0) {
          tbl = compptr->dc_tbl_no;
          if (! did_dc[tbl]) {
    	htblptr = & cinfo->dc_huff_tbl_ptrs[tbl];
    	if (*htblptr == NULL)
    	  *htblptr = jpeg_alloc_huff_table((j_common_ptr) cinfo);
    	jpeg_gen_optimal_table(cinfo, *htblptr, entropy->dc_count_ptrs[tbl]);
    	did_dc[tbl] = TRUE;
          }
        }
        /* AC needs no table when not present */
        if (cinfo->Se) {
          tbl = compptr->ac_tbl_no;
          if (! did_ac[tbl]) {
    	htblptr = & cinfo->ac_huff_tbl_ptrs[tbl];
    	if (*htblptr == NULL)
    	  *htblptr = jpeg_alloc_huff_table((j_common_ptr) cinfo);
    	jpeg_gen_optimal_table(cinfo, *htblptr, entropy->ac_count_ptrs[tbl]);
    	did_ac[tbl] = TRUE;
          }
        }
      }
    }

    /*
     * Initialize for a Huffman-compressed scan.
     * If gather_statistics is TRUE, we do not output anything during the scan,
     * just count the Huffman symbols used and generate Huffman code tables.
     */

    METHODDEF(void)
    start_pass_huff (j_compress_ptr cinfo, boolean gather_statistics)
    {
      huff_entropy_ptr entropy = (huff_entropy_ptr) cinfo->entropy;
      int ci, tbl;
      jpeg_component_info * compptr;

      if (gather_statistics)
        entropy->pub.finish_pass = finish_pass_gather;
      else
        entropy->pub.finish_pass = finish_pass_huff;

      if (cinfo->progressive_mode) {
        entropy->cinfo = cinfo;
        entropy->gather_statistics = gather_statistics;

        /* We assume jcmaster.c already validated the scan parameters. */

        /* Select execution routine */
        if (cinfo->Ah == 0) {
          if (cinfo->Ss == 0)
    	entropy->pub.encode_mcu = encode_mcu_DC_first;
          else
    	entropy->pub.encode_mcu = encode_mcu_AC_first;
        } else {
          if (cinfo->Ss == 0)
    	entropy->pub.encode_mcu = encode_mcu_DC_refine;
          else {
    	entropy->pub.encode_mcu = encode_mcu_AC_refine;
    	/* AC refinement needs a correction bit buffer */
    	if (entropy->bit_buffer == NULL)
    	  entropy->bit_buffer = (char *) (*cinfo->mem->alloc_small)
    	    ((j_common_ptr) cinfo, JPOOL_IMAGE, MAX_CORR_BITS * SIZEOF(char));
          }
        }

        /* Initialize AC stuff */
        entropy->ac_tbl_no = cinfo->cur_comp_info[0]->ac_tbl_no;
        entropy->EOBRUN = 0;
        entropy->BE = 0;
      } else {
        if (gather_statistics)
          entropy->pub.encode_mcu = encode_mcu_gather;
        else
          entropy->pub.encode_mcu = encode_mcu_huff;
      }

      for (ci = 0; ci < cinfo->comps_in_scan; ci++) {
        compptr = cinfo->cur_comp_info[ci];
        /* DC needs no table for refinement scan */
        if (cinfo->Ss == 0 && cinfo->Ah == 0) {
          tbl = compptr->dc_tbl_no;
          if (gather_statistics) {
    	/* Check for invalid table index */
    	/* (make_c_derived_tbl does this in the other path) */
    	if (tbl < 0 || tbl >= NUM_HUFF_TBLS)
    	  ERREXIT1(cinfo, JERR_NO_HUFF_TABLE, tbl);
    	/* Allocate and zero the statistics tables */
    	/* Note that jpeg_gen_optimal_table expects 257 entries in each table! */
    	if (entropy->dc_count_ptrs[tbl] == NULL)
    	  entropy->dc_count_ptrs[tbl] = (long *) (*cinfo->mem->alloc_small)
    	    ((j_common_ptr) cinfo, JPOOL_IMAGE, 257 * SIZEOF(long));
    	MEMZERO(entropy->dc_count_ptrs[tbl], 257 * SIZEOF(long));
          } else {
    	/* Compute derived values for Huffman tables */
    	/* We may do this more than once for a table, but it's not expensive */
    	jpeg_make_c_derived_tbl(cinfo, TRUE, tbl,
    				& entropy->dc_derived_tbls[tbl]);
          }
          /* Initialize DC predictions to 0 */
          entropy->saved.last_dc_val[ci] = 0;
        }
        /* AC needs no table when not present */
        if (cinfo->Se) {
          tbl = compptr->ac_tbl_no;
          if (gather_statistics) {
    	if (tbl < 0 || tbl >= NUM_HUFF_TBLS)
    	  ERREXIT1(cinfo, JERR_NO_HUFF_TABLE, tbl);
    	if (entropy->ac_count_ptrs[tbl] == NULL)
    	  entropy->ac_count_ptrs[tbl] = (long *) (*cinfo->mem->alloc_small)
    	    ((j_common_ptr) cinfo, JPOOL_IMAGE, 257 * SIZEOF(long));
    	MEMZERO(entropy->ac_count_ptrs[tbl], 257 * SIZEOF(long));
          } else {
    	jpeg_make_c_derived_tbl(cinfo, FALSE, tbl,
    				& entropy->ac_derived_tbls[tbl]);
          }
        }
      }

      /* Initialize bit buffer to empty */
      entropy->saved.put_buffer = 0;
      entropy->saved.put_bits = 0;

      /* Initialize restart stuff */
      entropy->restarts_to_go = cinfo->restart_interval;
      entropy->next_restart_num = 0;
    }

    /*
     * Module initialization routine for Huffman entropy encoding.
     */

    GLOBAL(void)
    jinit_huff_encoder (j_compress_ptr cinfo)
    {
      huff_entropy_ptr entropy;
      int i;

      entropy = (huff_entropy_ptr) (*cinfo->mem->alloc_small)
        ((j_common_ptr) cinfo, JPOOL_IMAGE, SIZEOF(huff_entropy_encoder));
      cinfo->entropy = &entropy->pub;
      entropy->pub.start_pass = start_pass_huff;

      /* Mark tables unallocated */
      for (i = 0; i < NUM_HUFF_TBLS; i++) {
        entropy->dc_derived_tbls[i] = entropy->ac_derived_tbls[i] = NULL;
        entropy->dc_count_ptrs[i] = entropy->ac_count_ptrs[i] = NULL;
      }

      if (cinfo->progressive_mode)
        entropy->bit_buffer = NULL;	/* needed only in AC refinement scan */
    }